{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":2},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":150,"n_cols":6,"rows_kept":150,"merged":[[0,1,0,5],[1,0,1,5],[114,0,114,5]],"flags":["formulas_cached_only"]}
[null,"化材学院基础实验低值易耗品"]
["安师大化材学院2017-2018学年第二学期玻璃仪器、小型设备招标计划"]
["序号","货品名称","规格","单位","采购数量","备注"]
[1,"USB延长线","1米","根",4]
[2,"表面皿","70mm","个",50]
[3,"玻棒","20cm","根",250]
[4,"玻璃棒","6mm*30cm","根",400]
[5,"不锈钢药刮","30cm","把",100]
[6,"布氏漏斗","100mm","个",10]
[7,"布氏漏斗","80mm","个",50]
[8,"布氏漏斗（带橡皮塞）","10ml","个",20]
[9,"布氏漏斗托密封胶圈","套","套",20]
[10,"层析柱","内径5cm","个",10,"磨口"]
[11,"称量纸","75*75","袋",100]
[12,"称量纸","100*100mm","袋",100]
[13,"磁子","A100","个",200]
[14,"磁子","A200","个",600]
[15,"磁子","A300","个",200]
[16,"磁子","A400","个",50]
[17,"刺型分馏柱","19#","个",10]
[18,"导气弯管",null,"个",20,"磨口"]
[19,"滴管","15cm","支",800]
[20,"滴瓶","60ml","个",40]
[21,"碘 量 瓶","50ml","个",100]
[22,"电极线","辰华CHI660系列工作站连接线--4接头","根",7]
[23,"顶空瓶","150ML","支",16]
[24,"定性滤纸","9cm","盒",100]
[25,"定性滤纸","12.5cm","盒",50]
[26,"定性滤纸","15cm","盒",50]
[27,"定性滤纸","18cm","盒",50]
[28,"分水器",null,"个",40,"磨口易坏"]
[29,"分液漏斗","125ml","个",30]
[30,"硅胶管","6*9/10m","盒",20]
[31,"核磁样品管",null,"个",30]
[32,"恒压滴液漏斗","125mL/19#","支",20]
[33,"缓冲球","旋转蒸发仪用24#转19#","个",3,"磨口"]
[34,"碱式滴定管","50mL","支",100]
[35,"刻度吸管","2ml","个",10]
[36,"刻度吸管","50ml","个",10]
[37,"空心玻璃塞","19#","支",80]
[38,"冷凝管夹",null,"个",150]
[39,"量   筒","50ml","个",100]
[40,"量筒","1000ml","支",10]
[41,"量筒","30cm*2.6cm ","支",10,"特制"]
[42,"量筒","100ml","支",100]
[43,"量筒","10ml","个",400]
[44,"螺口顶空盖","配150ML顶空瓶用","包",1,"50或100只"]
[45,"试管刷","小号","个",300]
[46,"试管刷","大号","个",300]
[47,"烧杯刷","50-100mL烧杯","个",200]
[48,"烧瓶刷","中号","个",200]
[49,"迷你量杯","30ml/只","支",50]
[50,"磨口90度弯管",null,"个",20,"看样定做"]
[51,"毛细管(两端不封)","0.5mm","筒",10,"看样定做"]
[52,"毛细管(一端封端)","0.5mm","筒",10,"看样定做"]
[53,"磨口毛细管","L=18.5cm","个",20]
[54,"凝固点套管","内管L=18cm       外管L=16cm","套",20]
[55,"启普发生器","125ml","个",30]
[56,"气相进样针","尖头，1微升","支",3]
[57,"球形冷凝管","19#  L=20cm","个",50]
[58,"球形冷凝管","19#  L=30cm","个",50]
[59,"乳胶管","6*9","米",200]
[60,"三角漏斗","90mm","支",100]
[61,"三角漏斗","90mm","支",100]
[62,"三角漏斗","40mm","个",70]
[63,"锥形瓶","150ml","支",30]
[64,"三口烧瓶","250ml/19","支",10]
[65,"烧杯","1000ml","个",100]
[66,"烧杯","100ml","个",600]
[67,"烧杯","500ml","个",60]
[68,"烧杯","250ml","个",100]
[69,"烧杯","50ml","个",600]
[70,"烧杯","150mL","个",200]
[71,"烧瓶夹",null,"个",200]
[72,"十字夹",null,"个",200]
[73,"石棉网","15cm/封边","个",200]
[74,"试管","15×150mm","支",1600]
[75,"试管","10×100mm","支",100]
[76,"试管夹",null,"个",50]
[77,"试管架（塑料）",null,"个",50]
[78,"输血管",null,"袋",2]
[79,"数据线","串口线，DB9孔(母)-DB9孔(母) ","根",5]
[80,"四氟搅拌杆","根","个",40]
[81,"四氟搅拌杆套","19#","个",40]
[82,"塑料盒","内侧60cm*40cm*15cm","个",5]
[83,"塑料盒","内侧40cm*30cm*15cm","个",8,"蛇形"]
[84,"酸式滴定管","50mL","支",100]
[85,"索氏提取器","250ml","个",5]
[86,"脱脂棉","500g","包",10,"磨口"]
[87,"温度计","200度","支",20]
[88,"温度计套管（19#）","19#","个",40]
[91,"橡皮塞","6号","公斤",2]
[92,"橡皮塞","2号","公斤",2]
[93,"橡皮塞","4号","公斤",2]
[94,"橡皮塞","7号","公斤",2]
[95,"橡皮塞","8号","公斤",2]
[96,"橡皮塞","10号","公斤",2]
[97,"橡皮塞","11号","公斤",3]
[98,"液相进样针","平头，20微升","个",4]
[99,"一次性滴管","5mL/100支/包","包",12,"磨口"]
[100,"有机相针式过滤器","孔径：0.22um;直径：13mm.","个",1000,"磨口"]
[101,"圆底烧瓶（19#/100ml）","19#/100ml","个",60,"磨口"]
[102,"圆底烧瓶（19#/25ml）","19#/25ml","个",50]
[103,"圆底烧瓶（19#/50ml）","19#/50ml","个",30]
[104,"长 滴 管","L=25cm","支",100]
[105,"真空尾接管19#","19#","个",10]
[106,"真空橡皮管（6×12mm）","6×12mm","kg",15]
[107,"蒸馏头","19#","个",10]
[108,"直形冷凝管","20cm/19#","只",20]
[109,"止水夹",null,"个",20]
[110,"锥形瓶","100ml","个",40]
[111,"紫外II型光谱照相版","9*24cm","盒",3]
[112,"自封塑料袋","12*17/6号","个",100]
[113,"棕色广口瓶","500mL","个",6,"备注"]
["小型设备"]
["序号","名称","参数、型号","单位","数量"]
[1,"混凝土可拆卸试模","100x100x100 mm3三联  钢制","套",20]
[2,"水泥胶砂试模","40*40*160三联     钢制","套",20]
[3,"混凝土抗裂试模","425*305*100砼抗裂试模    铸铁","套",20]
[4,"混凝土早期开裂刀口约束试模","800*600*100  铸铁","套",10]
[5,"水泥胶砂抗压夹具","40x40   铸铁","套",10]
[6,"电子秤","量程30kg 凹盘 液晶显示，带电池","台",3]
[7,"电子称","量程300kg","台",2]
[8,"水泥标准养护箱   ","SHBY-40型","台",1]
[9,"电动手持座式搅拌机","祈和KS-806S型 2.5L 400W纯铜电机  ","台",2]
[10,"水泥砂浆干缩试模","25*25*280mm 标配铜质测头","套",10]
[11,"水泥砂浆干缩试模","40*40*160mm 标配铜质测头","套",10]
[12,"新标准水泥胶砂限制膨胀率仪","BC156-300型 数显12.7mm千分表 测量范围156mm-305mm","台",5]
[13,"铜质测头","与砂浆干缩试模 25*25*280mm标配使用","个","6*20","上海医疗器械股份有限公司"]
[14,"铜质测头","与砂浆干缩试模 40*40*160mm标配使用","个","6*20","闽豹"]
[15,"浮标式氧气吸入器","YH.YX11D ","个",2,"万旌辉"]
[16,"工具套装","含（锂电钻、羊角锤、万用表、活动扳手、卷尺、剥线钳、水管钳、老虎钳、尖嘴钳、内六角扳手、锯子、精密批*4、棘轮手柄、一字起子、十字起子等）淘宝价格为368元","套",1,"Victor/胜利"]
[17,"平板车","71*48/400斤（小） 超静音","个",1]
[18,"万用表","数字万用表VC890","个",1]
[19,"电子天平","600g/0.01g","台",1]
[20,"水浴锅","6孔","台",1]
[21,"卷尺","5m","个",1]
[22,"激光黑白打印机","黑白激光","台",3]
[23,"熔点测定仪","X-6/带摄像头","台",2]
[24,"干湿吸尘吸水器","15-30L","台",2]
[25,"双层药品推车","不锈钢","只",2]
[26,"小拖车（软轮静音）","200斤","只",1]
[27,"数显磁力加热套","250ml","台",10]
[28,"电动搅拌机","JJ-1","台",10]
[29,"电冰箱","150-200","台",2]
[30,"纯水机","实验室小型","台",1,"常州市双杰测试仪器厂"]
[32,"喷漆面罩","粉末涂料用","只",20,"常州市双杰测试仪器厂"]
[33,"电子天平","600g/0.1g","个",14,"常州市双杰测试仪器厂"]
[34,"T200电子天平","Max=200g \ne=10d\nd=0.1g","个",3]
[35,"T500电子天平","Max=500g \ne=10d\nd=0.1g","个",3]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}